**10 Port Full Gigabit Intelligent Standard PoE Switch**

【Product Description】

###### 10 Port Full Gigabit Intelligent Standard PoE Switch, using high-quality high-speed network IC and the most stable POE chip, POE port meets 802.3af / 802.3at standard, this series of PoE Switch can be 10/100/1000M Ethernet. The network provides a seamless connection, and the PoE power port can automatically detect and power the powered devices that comply with the IEEE802.3af / IEEE802.3at standards. The non-POE device intelligently detects no power and only transmits data.

###### PoE is Power over Ethernet, which refers to the transmission of data signals to some IP-based terminals (such as IP phones, wireless access AP, network cameras, etc.), but also provides DC power for the device. Technically, these devices that receive DC power are called powered devices.

###### With simple and convenient installation and maintenance methods and rich business features, it helps users to build a safe and reliable high-performance network. It is mainly located in the core or convergence layer of user networks such as industrial parks, buildings, factories and mines, government agencies, and residential broadband; it can be widely used in Ethernet access scenarios such as small and medium-sized enterprises, Internet cafes, hotels, and schools.

###### 【Main Features】

* Support 8\* 10/100/1000M PoE Ports+2\* Gigabit SFP Ports;
* Ethernet Ports support 10/100/1000M self-adaptive;
* The AI mode is automatically enabled 10M speed for Ports 7-8 in Extend mode;
* Flow control mode: IEEE 802.3X standard for full duplex, and Back Pressure standard for half duplex;
* Zero configuration feature, automatically supplied to adaptive equipment;
* Panel indicator monitoring status and help failure analysis;
* With DIP switch, support Default and Extend modes;
* Support Surge protection: Common mode 4KV; ESD: Air 8KV, Contact 6KV.


【Application Environment】

* Metro Optical Broadband Network: Data network operators such as telecommunications, cable TV, and network system integration,etc.
* Broadband private network: Suitable for financial, government, oil, railway, electric power, public security, transportation, education and other industries
* Multimedia transmission: Integrated transmission of images, voice and data, suitable for remote teaching, conference TV, videophone and other applications
* Real-time monitoring: Simultaneous transmission of real-time control signals, images and data


【Specifications】

|  |  |
| --- | --- |
| **I/O Interface** | |
| Power | AC100-240V50/60Hz |
| Ethernet | 8\* Gigabit PoE Ports  2\* Gigabit SFP Ports |
| Chipset | 2\*RTL8367S  RTL8238B |
| Performance | |
| Bandwidth | 20Gbps |
| Pack forward rate | 14.88Mpps |
| Memory cache | 448Kb |
| MAC address | 2K |
| Jumbo Frame | 9216bytes |
| Transfer mode | Store and forward |
| MTBF | 100000 Hours |
| Standard | |
| Network Protocol | IEEE802.3 (10Base-T)  IEEE802.3u (100Base-TX)  IEEE802.3ab (1000Base-TX)  IEEE802.3x (Flow control)  IEEE 802.3z (Gigabit Ethernet Fiber Standard) |
| PoE Protocol | IEEE802.3af(15.4W)  IEEE802.3at(30W) |
| Industry Standard | EMI: FCC Part 15 CISPR (EN55032) class A  EMS: EN61000-4-2 (ESD),  EN61000-4-5 (Surge) |
| Network Medium | 10Base-T : Cat3, 4, 5 or above UTP(≤100m)  100Base-TX : Cat5 or above UTP(≤100m)  1000Base-TX : Cat5 or above UTP(≤100m) |
| Optical Medium | Multimode optical fiber: 50/125, 62.5/125, 100/140um  Single-mode optical fiber: 8/125, 8.7/125, 9/125, 10/125um |
| Certificate | |
| Safety Certification | CE, FCC, RoHS |
| Environment Standard | |
| Working Environment | Working Temperature: -10~50°C  Storage Temperature: -40~70°C  Working Humidity: 10%~90%, non-condensing  Storage Temperature: 5%~90%, non-condensing |
| Indicator | |
| LED Indicator | PWR (Power)，1-10 Green Light (Link&Data) |
| PWR | On: Powered on  Off: Powered off |
| 1-10 Green Light (Link&Data) | On: Link normal  Off: Link blocked  Flashing: Data transmitting |
| DIP Switch | Default: common mode, all interfaces can communicate with each other, the transmission distance is less than 100 meters, the transmission rate is 10/100/1000M adaptive; The port AI mode is disabled  Extend: Link extension mode, 7-8 ports force 10M, link 250M (enable POE watchdog) |
| Physical Specification | |
| Structure Size | Product Dimensions: 220\*161\*44mm  Package Dimensions: 315\*215\*85mm  Product N.W: 0.88kg  Product G.W: 1.38kg |
| Packing Info | Carton Dimensions: 445\*445\*335mm  Packing Quantity: 10 PCS  Packing Weight: 14.8KG |
| Power Voltage | Input Voltage: AC 100-240 V 50-60Hz  Supply Power: 52V2.3A |
| Power Consumption | ＜30W |
| Package List | Switch 1 pc, Power cord 1 pc, User manual 1 pc, Certification 1 pc |
| Order Info | |
| ZX900-AFG-82NS | 10 Port Full Gigabit Intelligent Standard PoE Switch |

**[Product Picture]**



**[Product Structure]**



**[Product Application]**

